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FITTING INSTRUCTIONS FOR MOCK CHIMNEY
HEALTH AND SAFETY

THESE INSTRUCTIONS ASSUME THAT THE CHIMNEY IS BEING FITTED BY A COMPETENT CONSTRUCTION WORKER, FAMILIAR WITH CURRENT HEALTH AND SAFTEY LEGISLATION AND IS EXPERIENCED WITH TIMBER ROOF CONSTRUCTION.

WARNING

Parts of the chimney may be sharp and the construction materials can cause irritation to the skin. It is recommended that protective gloves be worn when handling the chimney and a dust mask should be used when drilling through the saddle.

TV aerials or satellite dishes or any similar items must not be fitted to the chimney, doing so will invalidate the warranty. It is the builder’s responsibility to ensure that this information is passed onto the purchasers of the property.

Under no circumstances should the saddle be fitted using a nail gun or any attempt be made to pierce the saddle without first drilling the correct size of hole.

Any warranty will be void if the chimney is not fitted in the manner described in these instructions.

STEP 1
Ensure that the roof structure is properly secured in place before commencing work. Before the chimney is lifted into place measure the external dimensions of the saddle and fit additional structural timbers as required to ensure the all the fixing screws will connect the roof trusses or other structural timbers.

Sarking should now be fitted to the trusses if specified

The roof felt should be fitted in the conventional manner before the chimney is lifted into place.

Pre drill the 6mm diameter holes at 100mm centres through the raised flanges on the chimney saddle prior to lifting onto the roof.

STEP 2
Fit 2no lifting slings around the chimney using the choke sling method, below the level of the cope. Attach the slings to the lifting appliance and lift the chimney into place. The slings must not be attached or interfere with the cope or pot.
Align the chimney saddle with the roof trusses/additional timber, ensuring that the felt remains in place and is not damaged.

Lower the chimney into place

Under no circumstances must the cope or pot be used for lifting the chimney.

It is recommended that the lifting slings remain attached until the chimney has been secured to the roof structure.

STEP 3  
Fit the 6 x 100mm stainless steel screws and penny washers into the pre drilled holes in the saddle and securely fasten down.

STEP 4
On larger chimneys it may be necessary to fix additional timbers from the roof trusses down to the ceiling joists to spread the load. If in doubt please contact the supplier for advice.
In particularly exposed or windy locations additional fixings along with extra structural timbers may be required. If in doubt please contact the supplier for advice.

TILE LATHS
Tile laths should also be located as per a conventional chimney but must only be nailed around the saddle and not nailed through the saddle.

ROOF TILES

Tile as per a roof fitted with a conventional chimney.

LEAD FLASHING

Dress the pre fixed lead flashing down over the tiles below the chimney.
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